{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["初级Ａ（砌筑砖基础）","初级B（砌筑毛石基础）","初级Ｃ（清水墙砌筑）","中级Ａ（砌筑砖柱）","中级Ｂ（铺黏土砖室外路面）","中级Ｃ（砌筑空斗墙）","高级Ａ（砌筑干摆墙）","高级Ｂ（砌圆形砖烟囱）","高级Ｃ（发圆形砖券）"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"初级Ａ（砌筑砖基础）","index":0,"n_rows":17,"n_cols":8,"rows_kept":17,"merged":[[0,0,0,7],[1,1,1,7],[2,0,2,7],[4,0,7,0],[4,1,7,1],[4,6,7,6],[4,7,7,7],[8,0,14,0],[8,1,14,1],[8,6,14,6],[8,7,14,7],[16,0,16,1],[16,2,16,3],[16,4,16,5],[16,6,16,7]],"flags":["formulas_cached_only"]}
["建筑工种职业技能鉴定\n初级瓦工技能考试评分表(A卷)"]
[null,"砌筑砖基础"]
["单位                                姓名                  准考证号"]
["项目","项目配分","序号","技术要求及评分标准","配分","实测结果","实得分","备注"]
["质量要求","４0分",1,"砂浆饱满度８５％",10]
[null,null,2,"轴线偏差１０mm",10]
[null,null,3,"上下错缝、内外搭砌",10]
[null,null,4,"顶面标高±１５mm",10]
["操作要点","４0分",5,"检查放线",5]
[null,null,6,"标高修正",5]
[null,null,7,"摆底",10]
[null,null,8,"收退",5]
[null,null,9,"正墙",5]
[null,null,10,"检查",5]
[null,null,11,"节约材料",5]
["完成情况","20分",12,"全部完成",20]
["考评员 签字",{"$nulls":3},"实得总分"]

{"sheet":"初级B（砌筑毛石基础）","index":1,"n_rows":18,"n_cols":8,"rows_kept":18,"merged":[[0,0,0,7],[1,1,1,7],[2,0,2,7],[4,0,6,0],[4,1,6,1],[4,6,6,6],[4,7,6,7],[7,0,15,0],[7,1,15,1],[7,6,15,6],[7,7,15,7],[17,0,17,1],[17,2,17,3],[17,4,17,5],[17,6,17,7]],"flags":["formulas_cached_only"]}
["建筑工种职业技能鉴定\n初级瓦工技能考试评分表(B卷)"]
[null,"砌筑毛石基础"]
["单位                                姓名                  准考证号"]
["项目","项目配分","序号","技术要求及评分标准","配分","实测结果","实得分","备注"]
["质量要求","３0分",1,"轴线位移2０mm",10]
[null,null,2,"基顶标高±２５mm",10]
[null,null,3,"砌体厚度３０mm",10]
["操作要点","４0分",4,"拉结石设置",5]
[null,null,5,"检查放线",5]
[null,null,6,"摆底",5]
[null,null,7,"收退",5]
[null,null,8,"正墙",5]
[null,null,9,"检查",5]
[null,null,10,"填心砌法",5]
[null,null,11,"错缝搭砌",5]
[null,null,12,"第一层坐浆",5]
["完成情况","25分",13,"全部完成",25]
["考评员 签字",{"$nulls":3},"实得总分"]

{"sheet":"初级Ｃ（清水墙砌筑）","index":2,"n_rows":19,"n_cols":8,"rows_kept":19,"merged":[[0,0,0,7],[1,1,1,7],[2,0,2,7],[4,0,11,0],[4,1,11,1],[4,6,11,6],[4,7,11,7],[12,0,16,0],[12,1,16,1],[12,6,16,6],[12,7,16,7],[18,0,18,1],[18,2,18,3],[18,4,18,5],[18,6,18,7]],"flags":["formulas_cached_only"]}
["建筑工种职业技能鉴定\n初级瓦工技能考试评分表(C卷)"]
[null,"清水墙砌筑"]
["单位                                姓名                  准考证号"]
["项目","项目配分","序号","技术要求及评分标准","配分","实测结果","实得分","备注"]
["质量要求","４0分",1,"轴线位移１０mm",5]
[null,null,2,"标高±１５mm",5]
[null,null,3,"垂直度",5]
[null,null,4,"表面平整度５mm",5]
[null,null,5,"水平灰缝７mm",5]
[null,null,6,"水平灰缝厚度±８mm／每１０皮",5]
[null,null,7,"游丁走缝２０mm",5]
[null,null,8,"砂浆饱满度８０％",5]
["操作要点","４0分",9,"确定组砌方式",8]
[null,null,10,"排砖",8]
[null,null,11,"刮灰缝",8]
[null,null,12,"检查放线、皮数杆",8]
[null,null,13,"砖的选择",8]
["完成情况","20分",14,"全部完成",20]
["考评员 签字",{"$nulls":3},"实得总分"]

{"sheet":"中级Ａ（砌筑砖柱）","index":3,"n_rows":14,"n_cols":8,"rows_kept":14,"merged":[[0,0,0,7],[1,1,1,7],[2,0,2,7],[4,0,8,0],[4,1,8,1],[4,6,8,6],[4,7,8,7],[9,0,11,0],[9,1,11,1],[9,6,11,6],[9,7,11,7],[13,0,13,1],[13,2,13,3],[13,4,13,5],[13,6,13,7]],"flags":["formulas_cached_only"]}
["建筑工种职业技能鉴定\n中级瓦工技能考试评分表(Ａ卷)"]
[null,"砌筑砖柱"]
["单位                                姓名                  准考证号"]
["项目","项目配分","序号","技术要求及评分标准","配分","实测结果","实得分","备注"]
["质量要求","４0分",1,"轴线位移1０mm",8]
[null,null,2,"标高±１５mm",8]
[null,null,3,"表面平整度８mm ",8]
[null,null,4,"不许有包心砌法",8]
[null,null,5,"砂浆饱满度８０％",8]
["操作要点","３0分",6,"方柱定位",10]
[null,null,7,"组砌方式的确定",10]
[null,null,8,"检查（砌筑过程中的检查）",10]
["完成情况","３０分",9,"全部完成",20]
["考评员 签字",{"$nulls":3},"实得总分"]

{"sheet":"中级Ｂ（铺黏土砖室外路面）","index":4,"n_rows":15,"n_cols":8,"rows_kept":15,"merged":[[0,0,0,7],[1,1,1,7],[2,0,2,7],[4,0,8,0],[4,1,8,1],[4,6,8,6],[4,7,8,7],[9,0,12,0],[9,1,12,1],[9,6,12,6],[9,7,12,7],[14,0,14,1],[14,2,14,3],[14,4,14,5],[14,6,14,7]],"flags":["formulas_cached_only"]}
["建筑工种职业技能鉴定\n中级瓦工技能考试评分表(Ｂ卷)"]
[null,"铺黏土砖室外路面"]
["单位                                姓名                  准考证号"]
["项目","项目配分","序号","技术要求及评分标准","配分","实测结果","实得分","备注"]
["质量要求","４0分",1,"砖缝宽度≤５mm",8]
[null,null,2,"错缝长度　砖长１／３～１／２",8]
[null,null,3,"相邻两块高低差1.5mm",8]
[null,null,4,"表面平整度８mm",8]
[null,null,5,"5m长缝格平直8mm",8]
["操作要点","４0分",6,"排砖",10]
[null,null,7,"砂垫层刮平　压实　找平",10]
[null,null,8,"挂线　铺砌",10]
[null,null,9,"填缝",10]
["完成情况","20分",10,"全部完成",20]
["考评员 签字",{"$nulls":3},"实得总分"]

{"sheet":"中级Ｃ（砌筑空斗墙）","index":5,"n_rows":16,"n_cols":8,"rows_kept":16,"merged":[[0,0,0,7],[1,1,1,7],[2,0,2,7],[4,0,9,0],[4,1,9,1],[4,6,9,6],[4,7,9,7],[10,0,13,0],[10,1,13,1],[10,6,13,6],[10,7,13,7],[15,0,15,1],[15,2,15,3],[15,4,15,5],[15,6,15,7]],"flags":["formulas_cached_only"]}
["建筑工种职业技能鉴定\n中级瓦工技能考试评分表(C卷)"]
[null,"砌筑空斗墙"]
["单位                                姓名                  准考证号"]
["项目","项目配分","序号","技术要求及评分标准","配分","实测结果","实得分","备注"]
["质量要求","４0分",1,"轴线位移",7]
[null,null,2,"标高",7]
[null,null,3,"垂直度",7]
[null,null,4,"表面平整度",7]
[null,null,5,"水平灰缝平直度",6]
[null,null,6,"应砌实体部位",6]
["操作要点","４0分",7,"检查放线",10]
[null,null,8,"确定组砌方式",10]
[null,null,9,"材料节约",10]
[null,null,10,"排砖",10]
["完成情况","20分",11,"全部完成",20]
["考评员 签字",{"$nulls":3},"实得总分"]

{"sheet":"高级Ａ（砌筑干摆墙）","index":6,"n_rows":12,"n_cols":11,"rows_kept":12,"merged":[[0,0,0,11],[1,1,1,11],[2,0,2,11],[3,4,3,8],[4,9,7,9],[4,10,7,10],[8,9,10,9],[8,10,10,10],[11,0,11,2],[11,3,11,8],[11,9,11,10]],"flags":["formulas_cached_only"]}
["建筑工种职业技能鉴定\n高级瓦工技能考试评分表(Ａ卷)"]
[null,"砌筑干摆墙"]
["单位                                姓名                  准考证号"]
["序号","测定项目","技术要求及评分标准","配分","实测结果",{"$nulls":4},"实得分","备注"]
[1,"砖加工","允许偏差：长±２mm,宽±２mm，厚±１mm，超过规定数值无分",10]
[2,"排砖","丁砖应在三顺的中间，不得有七分头．排砖不符合要求、有破活无分",15]
[3,"墙面平整度","允许偏差±１mm,超过者每处扣除mm，三处以上或一处超过１．５mm无分",20]
[4,"操作工艺","按工艺流程操作，符合工艺标准满分，不符合者无分",20]
[5,"观感","墙面整齐、清洁、美观给满分；否则酌情扣分",15]
[6,"安全生产文明施工","发生工伤事故无分，活完场不清无分",10]
[7,"工效","按时完成满分，超过规定时间４０min无分；提前完成酌情加分，超时在４０min之内，酌情扣分",10]
["合计",null,null,"实得总分"]

{"sheet":"高级Ｂ（砌圆形砖烟囱）","index":7,"n_rows":15,"n_cols":11,"rows_kept":15,"merged":[[0,0,0,11],[1,1,1,11],[2,0,2,11],[3,4,3,8],[4,9,7,9],[4,10,7,10],[11,9,13,9],[11,10,13,10],[14,0,14,2],[14,3,14,8],[14,9,14,10]],"flags":["formulas_cached_only"]}
["建筑工种职业技能鉴定\n高级瓦工技能考试评分表(Ｂ卷)"]
[null,"砌圆形砖烟囱"]
["单位                                姓名                  准考证号"]
["序号","测定项目","技术要求及评分标准","配分","实测结果",{"$nulls":4},"实得分","备注"]
[1,"选砖","性能指标达不到要求无分（包括加工的砖）",5]
[2,"水平灰缝饱满度","标准９５％工资，工资低于标准每处扣除分，超过三处无分",15]
[3,"组砌方法","不符合要求、排砖错误无分",10]
[4,"灰缝","立缝里口不小于５mm,外口不大于１５mm，水平灰缝累计误差１０mm；在砌体顶面检查，每一处超过扣１分，三处以上无分",15]
[5,"任何截面半径","允许偏差３０mm，超过者每处扣１除分，三处以上及一处超过６０mm者无分",15]
[6,"囱壁内外表面局部凹凸不平","允许偏差３０mm，超过者每处扣１除分，三处以上及一处超过６０mm者无分",10]
[7,"中线垂直度","允许偏差３５mm，超过者酌情扣分",5]
[8,"勾缝","勾缝形式正确，勾缝深度适宜，墙面清洁给满分，否则酌情扣分",5]
[9,"安全生产文明施工","发生工伤事故无分，活完场不清无分",10]
[10,"工效","按时完成满分，超过规定时间４０min无分；提前完成酌情加分，超时在４０min之内，酌情扣分",10]
["合计",null,null,"实得总分"]

{"sheet":"高级Ｃ（发圆形砖券）","index":8,"n_rows":14,"n_cols":11,"rows_kept":14,"merged":[[0,0,0,11],[1,1,1,11],[2,0,2,11],[3,4,3,8],[4,9,7,9],[4,10,7,10],[10,9,12,9],[10,10,12,10],[13,0,13,2],[13,3,13,8],[13,9,13,10]],"flags":["formulas_cached_only"]}
["建筑工种职业技能鉴定\n高级瓦工技能考试评分表(Ｃ卷)"]
[null,"发圆形砖券"]
["单位                                姓名                  准考证号"]
["序号","测定项目","技术要求及评分标准","配分","实测结果",{"$nulls":4},"实得分","备注"]
[1,"选砖","选砖不符合要求无分",5]
[2,"排砖起拱","砖块数为单数，排砖符合要求满分，不符合要求无分",10]
[3,"平整度","允许偏差５mm，超过５mm每处扣１分，三处以上或一处超过８mm无分",10]
[4,"灰缝","灰缝应饱满，外口灰缝缝１５～２０mm，内口灰缝５～８mm，不符合要求的酌情扣扣３～１２分",15]
[5,"弧度","弧度应一致，不一致者无分",15]
[6,"清水墙面","刮缝深度１０～１２mm，墙面清洁美观不符合要求者酌情扣２～８分",10]
[7,"操作方法","符合工艺标准满分，不符合工艺要求无分",15]
[8,"安全生产文明施工","发生工伤事故无分，活完场不清无分",10]
[9,"工效","按时完成满分，超过规定时间３０min无分；提前完成酌情加分，超时在３０min之内，酌情扣分",10]
["合计",null,null,"实得总分"]